**MR.00 Series Specifications**

|  |
| --- |
| MR.00 is intended for the swing drive of mobile cranes. |

Technical characteristics:

|  |
| --- |
| MP.00 is intended for the swing drive of mobile cranes. |

Technical characteristics:

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Designation | Application | Gearbox parameters | | | | Motor displacement, ccm |
| ratio | torgue, Nm | input speed, max rpm | output speed, max rpm |
| MP.00.01 | mobile crane, 16…25t | 63.1 | 3646 | 1200 | 19 | 112 |
| MP.00.02 | mobile crane, 32…40t | 63.1 | 3646 | 1200 | 19 | 56 |
| MP.00.03 | mobile crane, 16…25t | 63.1 | 3646 | 1200 | 19 | 112 |