**COMPRESSORS**

Air pump group acting by a hydraulic piston motor, variable or fixed displacement, for having an easy and correct RPM adjustment. On request it is also possible to add a security valve that limited maximum oil flow in input avoiding possible exceeding RPM.

Hydraulic motors from 6cc to 14cc or from 21cc are connected by a coupling.  
The group is suitable for the use of air tools, for workshop machine builder, for the agricultural field and for all the constructors that want to simplify the installation of air group.   
Engine cooling is done by an electrical fan 12 or 24 Volts. We can supply a compact air valves group that can be putted fastly for the complete air control.