**Design:**

Groups generators and welders driven by a hydraulic piston motor, variable displacement for an easy and correct speed control, manual and also with electronic card, with Hertz automatic control at various of hydraulic performance and the required power.  
Hydraulic motor allow to use oil flow from 22 to 42 l/min, in addition it can be include limitation flow valves for superior oil quantity, maximum pressure valve and ON-OFF directional valve solenoid operated on request.   
This group is suitable for fitters workshop wagons, in the agricultural field, and for all manufacturers who want to simplify the installing an generator on its packing machine control board Hertz.

**Current Performance**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **AVAILABLE VOLTAGES** | 48 | 220 | 380 | AMPERE |
| **INGRESS PROTECTION RATING** | IP 23 | IP 23 | IP 23 | IP 23 |
| **KVA 220 VOLT** | Upon Request | 5/7/10 |  |  |
| **KVA 380 VOLT** |  |  | 7/10/16 |  |
| **WELDERS** |  |  |  | 220/300 |