**Design:**

The variable-displacement axial piston motors have been designed to work both in an open and closed circuit.  
Control sytems actually available are making easy to use these motors in any applications for industrial and mobile field.  
Available control systems are:

* 12V electrical control
* 24V electrical control
* Remote Hydraulic servo control

**Technical Features:**

