**Design:**

W0 14 series is a family of variable displacement axial piston pumps for use in closed circuits with housing and distributor cover in aluminium. The displacement is continuously variable by means of a tilting swash plate, and the oil flow direction is reversible.  
  
**Features:**

The following range of controls is available:

* Manual without zeroing
* Manual with zeroing

One through drive option for auxiliary pump mounting and two options are available:

* Through drive - Bosch Gr.1

Peak operations must not excide 1% of every minute.   
A simultaneous maximum pressure and maximum speed are not recommended.  
  
  
**Technical Specifications:**  
