Filter

Special Filter used for Hydraulic Transmission.

Suction and Return in only one filter with pressurization valve and mounting in line.

**Technical Specifications:**

|  |  |  |
| --- | --- | --- |
| Max Pressure | Bar | 12 |
| Oil Flow Rate | l/min | 150 |
| Weight | Kg | 5 |