Description

**SCP 012-130 ISO is a series of piston pumps with a fixed displacement for mobile and stationary hydraulics.**

SCP 012-130 ISO covers the entire displacement range 12-130 cmᶟ ⁄rev. at a maximum pressure of 400 bar. The pump´s well dimensioned, double tapered roller bearings permit high shaft loads and lead to excellent speed characteristics. The pump is drained externally. It is speed-optimised and therefore supplied for either left (L) or right (R) rotation direction.

Product benefits

• High maximum speed while maintaining low noise levels

• Smooth operation over the entire speed range

• Long life due to high demands on material selection, such as bearings, seals, etc.

