Description

**The Sunfab variable displacement pump with its rugged construction is designed for direct mounting at the auxiliary drive (P.T.O.) of commercial vehicles.**

With a max. displacement of 130 cm3/rev. and a peak pressure of 450 bar it is suited for many applications. This is complemented by the high self priming rate and the low noise level. The pump delivery flow is dependent on the present drive speed and geometric displacement. The flow is adjustable in a range between 0 and Qmax.

Product Benefits

• Short reaction time when resetting the flow

• Compact installation dimensions

• High working pressure level allowed

• Externally drained for best cooling

• Rugged construction and long service life

• Low noise emission

• High power-to-weight-ratio

