**Technical characteristics:**

|  |  |
| --- | --- |
| Parameter | Value |
| Inlet pressure, MPa - max | 20 |
| Outlet pressure (reduced), can be changed in proportion to pedal rotation angle, MPa - max | 6 |
| Working fluid flow, l/min - max | 70 |
| Weight, kg | 5 |