**MF Series Specifications**

**Purpose:**

Hydraulic motors MF.0.90 were developed on request of foreign consumers. Hydraulic motors MF.0.90 were initially intended for use in set with hydrostatic transmission of truck mounted concrete mixers. At present this series of hydraulic motors is widely used in hydraulic drives of mobile machinery f.i. in road rollers.

**Working displacement:**71, 80, 90 ccm/rev

**Design:**

- min overall dimensions in its class

- min weight in its class

- one side location of working lines

- mounted-in rotation speed sensor

Further development of MF series is carried out by the plant: hydraulic motors with working displacement 112cc/rev. on the base of the introduced design.