**Design:**

The fixed-displacement axial piston motors feature a swashplate-system and may operate in either closed or open circuit.  
Proper selection of materials and the use of steel cylinder blocks with inserted bushings guarantee the highest performance of the PWG S.r.l. motors, in terms of max. speed and working pressure.  
  
**Features:**

* Exceptionally high power/weight ratio
* Excellent volumetric and mechanical efficiency
* Long life
* Compact design
* Exchange valve fitted as optional.

**Technical Features:**

