Description

**SCP 012-108 SAE is a series of piston pumps with a fixed displacement for demanding mobile hydraulics.**

Sunfab SCP 012-108 SAE pumps are equipped with shafts and flanges according to the SAE-B and SAE-C standard. They are available in the range from 12-108 cmᶟ. It is a modern, compact pump which meets the market´s high demands on flow performance, pressure, efficiency and small installation dimensions.  
The pump is either mounted directly on the power take-off or on a frame bracket via an intermediate shaft.

Product Benefits

• High maximum speed while maintaining low noise levels

• Smooth operation over the entire speed range

• Long life due to high demands on material selection, such as bearings, seals, etc

• O-rings on all contact surfaces as well as double shaft seals eliminate oil leakage from the pump and power take-off

Technical Specifications

